{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["CALCULATION EASYFLEX"],"not_rendered":{"images":6,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"CALCULATION EASYFLEX","index":0,"n_rows":43,"n_cols":11,"rows_kept":43,"merged":[[0,0,0,10],[1,0,1,10],[2,0,2,10],[3,0,3,1],[3,8,6,8],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[8,8,9,8],[9,0,9,1],[10,0,10,10],[14,0,14,10],[15,0,15,10],[19,0,19,10],[20,0,20,10],[24,0,24,10]],"flags":["formulas_cached_only"]}
[]
["EASYFLEX CALCULATION SHEET"]
[]
["EASY FLEX GLIJDERS",null,"Afstand",null,null,"Aantal glijders","Lengte Mtr","Voor railmaat"]
["FES 50%",null,{"v":8,"d":"8.00"},null,null,500,{"v":40,"d":"40.00"},30.15]
["FES 80%",null,6.03,null,null,500,30.15,30.15]
["FES 100%",null,{"v":5.4,"d":"5.40"},null,null,500,{"v":27,"d":"27.00"},{"v":27,"d":"27.00"}]
[]
["EASYFLEX BAND",{"$nulls":5},"Op rol (mtr)","Op rol (cm)"]
["Transparant wit",{"$nulls":5},100,{"v":10000,"d":"10,000"}]
["EASY FLEX 60% (8,00 cm carrier distance)"]
["Rail size","FES 60%","Desired Wave","Tape Length³","Curtain","Curtain","Carriers","Tape","Track","Carriers","Tape"]
["in CM","Carriers¹","Depth in cm ²","Curtain Width","Fullness","Stacking ⁴","No. Of Rolls","No. Of Rolls","Quantity","No. Of Rolls","No. Of Rolls"]
[1000,126,10,1260,{"v":1.26,"d":"126%"},177.09999999999997,{"v":0.252,"d":"0.2520"},{"v":0.126,"d":"0.1260"},1,{"v":0.252,"d":"0.2520"},{"v":0.126,"d":"0.1260"}]
["Calculation for single curtain only, for center closing curtains, divide final rail size by 2 and insert this nummer as rail size in cm."]
["EASY FLEX 80% (6,03 cm carrier distance)"]
["Rail size","FES 80%","Desired Wave","Tape Length³","Curtain","Curtain","Carriers","Tape","Track","Carriers","Tape"]
["in CM","Carriers¹","Depth in cm ²","Curtain Width","Fullness","Stacking ⁴","No. Of Rolls","No. Of Rolls","Quantity","No. Of Rolls","No. Of Rolls"]
[1000,166,10,1660,{"v":1.66,"d":"166%"},233.09999999999997,{"v":0.332,"d":"0.3320"},{"v":0.166,"d":"0.1660"},1,{"v":0.332,"d":"0.3320"},{"v":0.166,"d":"0.1660"}]
["Calculation for single curtain only, for center closing curtains, divide final rail size by 2 and insert this nummer as rail size in cm."]
["EASY FLEX 100% (5,40 cm carrier distance)"]
["Rail size","FES 100%","Desired Wave","Tape Length³","Curtain","Curtain","Carriers","Tape","Track","Carriers","Tape"]
["in CM","Carriers¹","Depth in cm ²","Curtain Width","Fullness","Stacking ⁴","No. Of Rolls","No. Of Rolls","Quantity","No. Of Rolls","No. Of Rolls"]
[1000,186,10,1860,{"v":1.86,"d":"186%"},261.09999999999997,{"v":0.372,"d":"0.3720"},{"v":0.186,"d":"0.1860"},1,{"v":0.372,"d":"0.3720"},{"v":0.186,"d":"0.1860"}]
["Calculation for single curtain only, for center closing curtains, divide final rail size by 2 and insert this nummer as rail size in cm."]
[]
[null,"= Required fields to fill in or correct manually"]
[]
["¹ Safety Margin : "]
["1 additional carrier automatically added for even number of carriers."]
[]
["² Wave Depth :"]
["Also known as total curtain depth; distance from frontside of the curtain till the backside of the curtain. This also determines the pelmet size."]
[]
["³ Safety Margin:"]
["Multiply the number of carriers by the desired wave depth, giving you the actual length of the tape and width of the curtain"]
["The length of the tape determines the quantity of curtain fabric needed per system."]
["Add enough fabric to create the hems at both sides of the curtain."]
[]
["⁴ Curtain Stacking:"]
["Based on manual tracks KS, DS or CS; without master carrier; one-way or middle closing."]
[]
["Note : no rights can be derived from this calculation sheet."]